**SECTION 107**

**LEGAL RELATIONS AND RESPONSIBILITY TO PUBLIC**

Standard Modifications

**107-1.02 PERMITS, LICENSES AND TAXES.**

*DELETE Item 1. under the paragraph beginning with “In addition…” and REPLACE with the following:*

1. Contact all government agencies having possible or apparent permit authority over that area, which may include, but are not limited to:
	1. US Army Corps of Engineers
	2. Alaska Department of Fish and Game
	3. Alaska Department of Environmental Conservation
	4. Alaska Department of Natural Resources
	5. Alaska Department of Transportation
	6. Matanuska-Susitna Borough
	7. All other tribal, federal, state, or local authorities;

**107-1.06 SANITARY, HEALTH, SAFETY PROVISIONS.** *ADD the following*: The Contractor shall provide and maintain restroom facilities for Contractor’s employees and Owner’s representatives at all work sites.

**107-1.11 PROTECTION AND RESTORATION OF PROPERTY AND LANDSCAPE.**

Under Item 2. Material Disposal Sites *add the following*:

Material disposal sites on private property adjacent to the project, shall be blended into the surrounding contours and permanently stabilized. No slope shall exceed 2:1, unless approved by the Engineer.

Under Item 7. Protected areas, *add the following*: All clearing and/or grubbing activities shall take place outside of the Migratory Bird Treaty Act (MBTA) window as determined by the U.S. Fish and Wildlife Service (FWS) under the website publication for the construction year:  [https://www.fws.gov/alaska-bird-nesting-season](https://linkprotect.cudasvc.com/url?a=https%3a%2f%2fwww.fws.gov%2falaska-bird-nesting-season&c=E,1,W4M5BxfzQ7khMHzInygoEc6lMnogZEliBrirwkDHi5BGEj0oYmeea7v3b1j_cLNoT3U6P0npP2Pi5s3MeeRf6pSgIwJGHw3fVdmicLC5Qe4-5-oK65JiDQ,,&typo=1)

**107-1.16** *Delete and replace with the following:*

**107-1.16 CONTRACTOR'S RESPONSIBILITY FOR UTILITY PROPERTY AND SERVICES.**

Where the Contractor's operations meet any of the following conditions, the Contractor shall advise the owning Utility in writing at least 24 hours in advance of the work.

1. Operations anticipated to be within 10 feet of an overhead electrical line.
2. Operations anticipated to be within 3 feet of an underground electrical line according to locates provided by the owning Utility.
3. Operations requiring use of equipment, which is capable of coming within 10 feet of an overhead electrical line.

The notice shall indicate the location and duration of the work to be performed.

The Contractor shall provide an attendant whose sole responsibility is to perform as a safety observer while equipment is operating such that any part is capable of reaching within 15 feet of an overhead line.

Providing a safety observer for overhead electrical facilities, or a cable watch for buried electrical facilities, will not be paid for separately, but will be subsidiary to the item(s) of work being performed requiring these services.

MSB 051823